{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":15,"rows_kept":35,"cut":false,"hidden":false,"merged":[[16,2,16,6],[16,7,16,11],[17,2,17,6],[24,2,24,6],[24,7,24,11],[22,2,22,6],[23,2,23,6],[22,7,22,11],[23,7,23,11],[21,2,21,6],[18,2,18,6],[17,7,17,11],[18,7,18,11],[21,7,21,11],[20,2,20,6],[20,7,20,11],[19,2,19,6],[19,7,19,11],[15,2,15,6],[13,7,13,11],[14,7,14,11],[15,7,15,11],[8,7,8,11],[9,7,9,11],[13,2,13,6],[14,2,14,6],[12,2,12,6],[12,7,12,11],[0,0,0,13],[2,2,2,6],[2,7,2,11],[3,2,3,6],[3,7,3,11],[1,13,1,14],[4,7,4,11],[5,2,5,6],[5,7,5,11],[9,2,9,6],[4,2,4,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[6,7,6,11],[7,7,7,11],[27,2,27,6],[27,7,27,11],[25,2,25,6],[25,7,25,11],[26,2,26,6],[26,7,26,11],[30,2,30,6],[30,7,30,11],[10,2,10,6],[10,7,10,11],[11,2,11,6],[11,7,11,11],[29,2,29,6],[29,7,29,11],[28,2,28,6],[28,7,28,11]],"flags":["formulas_cached_only"]}
["Highlander R7780RP-1不具合項目一覧"]
[{"$nulls":13},"2005/06/03 現在"]
["項番","機能","項目",{"$nulls":4},"状況",{"$nulls":4},"ACE担当","RSO担当","ステータス"]
[1,"IPL","CF Boot",{"$nulls":4},"認識しない CF がある。",{"$nulls":4},"佐久間","福島／佐野","Debug 中"]
[2,{"$nulls":6},"Boot しない CF がある。",{"$nulls":4},"佐久間","福島／佐野","Debug 中"]
[3,null,"Network Boot (ASIX 88796L)",{"$nulls":4},"ASIX 88976L が動作しない",{"$nulls":4},"佐久間","福島／佐野","済み"]
[4,{"$nulls":6},"ASIX 88796L Kernel boot サポート",{"$nulls":4},"佐久間",null,"済み"]
[5]
[6]
[7,"Kernel","RPCIRP-1 ボード",{"$nulls":4},"RTL8110S-32 EEPROM が正しく読めない",{"$nulls":4},"細川","福島／佐野","済み"]
[8,{"$nulls":6},"PCI1520 CardBus 動作検証",{"$nulls":4},"細川","福島／佐野","Debug 中"]
[9,{"$nulls":6},"汎用 PCI ポート動作確認",{"$nulls":4},"細川","福島／佐野","済み"]
[10,null,"RDBRP-1 ボード",{"$nulls":4},"ASIX 88796L が動作しない",{"$nulls":4},"細川","福島／佐野","済み"]
[11,{"$nulls":6},"ASIX 88796L の MAC Address が取得出来ない",{"$nulls":4},"細川",null,"済み"]
[12,null,"Booting",{"$nulls":4},"Boot 中に Register Dump する",{"$nulls":4},"細川／佐久間","福島／佐野","Debug 中"]
[13,{"$nulls":6},"Boot 中に固まる",{"$nulls":4},"細川／佐久間","福島／佐野","Debug 中"]
[14,{"$nulls":6},"Partner-Jet 接続中頻繁に固まる",{"$nulls":4},"細川／佐久間","福島／佐野","未着手"]
[15,null,"SH7780 エラッタ",{"$nulls":4},"INTC のエラッタ対応",{"$nulls":4},"細川","坂戸","済み"]
[16,null,"32 Bit Address 拡張",{"$nulls":4},"32 Bit Address 拡張モード動作検証",{"$nulls":4},"細川","坂戸","未着手"]
[17,null,"ATA/IDE",{"$nulls":4},"CF, SATA でエラーが発生する場合がある",{"$nulls":4},"細川／佐久間",null,"Debug 中"]
[18]
[19,"Rootfs","/etc/rc.d/rc.sysinit",{"$nulls":4},"wait コマンドが終了しない",{"$nulls":4},"菊武",null,"未着手"]
[20,null,"Network パフォーマンス測定",{"$nulls":4},"RTL8110S-32 パフォーマンス測定",{"$nulls":4},"細川／菊武",null,"未着手"]
[21,null,"SATA パフォーマンス測定",{"$nulls":4},"Sil2112 パフォーマンス測定",{"$nulls":4},"細川／菊武",null,"未着手"]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[]
["※：項番１，２，１２，１３，１７は、「Debug 中」ですが、2005/06/02 ハードウェア改修を行い、対処済みです。只今、検証中。"]
["※：項番１５は、IRLn を保持しない（SH-4と同じ）モードを使用しています。"]
["※：項番８は、CardBus 対応デバイスを装着出来ない為、検証出来ません。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}