{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["リリース図","結合前（編集用）"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"リリース図","index":0,"n_rows":77,"n_cols":82,"rows_kept":77,"cut":false,"hidden":false,"merged":[[60,70,64,76],[66,70,70,76],[56,81,72,92],[56,15,72,26],[60,43,62,50],[64,43,66,50],[68,43,70,50],[58,55,58,75],[61,33,62,40],[64,33,65,40],[66,54,70,60],[66,62,70,68],[12,3,20,11],[60,54,64,60],[60,62,64,68],[39,15,42,26],[44,15,47,26],[49,15,52,26],[13,15,19,26],[48,31,50,37],[48,39,50,45],[48,47,50,53],[13,29,19,78],[13,81,19,92],[39,81,42,92],[44,81,47,92],[49,81,52,92],[47,75,51,78],[40,31,42,37],[23,63,27,69],[23,71,27,76],[34,31,35,64],[40,39,42,45],[40,47,42,53],[44,31,46,37],[44,39,46,45],[44,47,46,53],[23,55,27,61],[4,3,7,79],[23,31,24,52],[58,43,58,50],[38,31,38,53],[38,57,38,64],[40,57,42,64],[44,57,46,64],[48,57,50,64],[40,75,44,78],[2,3,3,52],[76,63,78,94],[36,15,37,26],[33,15,34,26],[9,13,10,70],[67,33,68,40],[70,33,71,40],[58,33,59,40],[56,29,72,30],[34,81,35,92]],"flags":["formulas_cached_only"]}
[]
[]
[null,null,null,"Customer product"]
[]
[null,null,null,"Android custom application (Dalvik App.)"]
[]
[]
[]
[]
[{"$nulls":13},"  RMC (or others) turn-key APP platform"]
[]
[]
[null,null,null,"Production\nCTS"]
[{"$nulls":15},"limited CTS\non APP board",{"$nulls":13},"Android common code\n( ASIS of AOSP )",{"$nulls":51},"limited CTS\non REF board"]
{"$rows_empty":9}
[{"$nulls":31},"Android framework & porting layer",{"$nulls":23},"Display",{"$nulls":7},"Stagefright",{"$nulls":7},"Modem"]
{"$rows_empty":9}
[{"$nulls":15},"on-APP board device"]
[{"$nulls":31},"on-chip device driver",{"$nulls":49},"on-REF board device"]
[]
[{"$nulls":15},"touch panel"]
[]
[{"$nulls":31},"Generic IP driver",{"$nulls":25},"Unique IP"]
[{"$nulls":15},"connectiivity",{"$nulls":65},"refernce camera"]
[{"$nulls":31},"INT",{"$nulls":7},"USB",{"$nulls":7},"LCD",{"$nulls":9},"VCP",{"$nulls":17},"SH CPU"]
[]
[]
[]
[{"$nulls":15},"sensor",{"$nulls":15},"TIMER",{"$nulls":7},"MTD",{"$nulls":7},"I2C",{"$nulls":9},"SPU/SPX",{"$nulls":23},"key / LED"]
[]
[]
[{"$nulls":75},"Modem"]
[{"$nulls":31},"DMA",{"$nulls":7},"MMC/SD",{"$nulls":7},"ALSA",{"$nulls":9},"SGX"]
[{"$nulls":15},"PMIC",{"$nulls":65},"PMIC"]
[]
[]
[]
[]
[]
[]
[{"$nulls":15},"Platform\nSupport\nCode for\nAPP Refernce\n( ex. Kota )",{"$nulls":13}," uboot",{"$nulls":51},"Platform\nSupport\nCode for\nSPF Refernce"]
[]
[{"$nulls":33},"kernel core",{"$nulls":9},"CPU ARCH",{"$nulls":11},"kernel common framework"]
[]
[{"$nulls":43},"ARM CA15",{"$nulls":10},"GPIO",{"$nulls":7},"CLOCK",{"$nulls":7},"PINMUX"]
[{"$nulls":33},"MM"]
[]
[]
[{"$nulls":33},"PM",{"$nulls":9},"ARM CA9"]
[]
[{"$nulls":54},"Runtime PM",{"$nulls":7},"Security",{"$nulls":7},"device tree"]
[{"$nulls":33},"scheduler"]
[{"$nulls":43},"ARM CA7"]
[]
[{"$nulls":33},"SMP/UP"]
[]
[]
[]
[]
[]
[{"$nulls":63},"SPF Linux common platform"]

{"sheet":"結合前（編集用）","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[[39,31,41,37]],"flags":["formulas_cached_only"]}